**Assumptions on the ambiguity of the window lifter requirement**

Due to the nature of the requirements some assumptions must be made in order to regulate the “holes” in the requirements.

In the requirements the requirement with the id 12, it states **“UP <500 msec the window shall UP until get totally CLOSED automatically. (Function one touch)”**, it doesn’t specified if while the automatic mode is functioning and press another button the automatic must cancel, in my assumption of the functionality the automatic mode must continue until gets totally open or closed, this is due to the mode mi design works and for how the manual mode works.